Torque Stick Policy

Effective immediately the Service Department will be required to use the supplied Torque Stick on any and all tires and wheels mounted on a vehicle. These are to be used only to install the tires (not remove) them. These are preset to torque the lug nuts only to 80lbs. The proper torque needs to be achieved by using a torque wrench.

There are enough supplied to cover every Tech, and Foreman in the shop. These are property of 4WP, NOT THE TECHS. If they leave we need to get them back.

The purpose of this is so the tech will not over-torque the wheels causing an unsafe condition.

**I need every Shop Leader to make sure to verify that you received the correct amount of Torque Sticks, sign this sheet and fax it back to me.**

Signature\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_Store\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Fax # 310-667-9146

Mark Allen